 
Other Stuff (MATLAB)
===========================================================================
 
   May 21, 2018
 
   The extensive scope of the Mice system's functionality includes features
   the average user may not expect or appreciate, features NAIF refers to
   as "Other Stuff." This workbook includes a set of lessons to introduce
   the beginning to moderate user to such features.
 
   The lessons provide a brief description to several related sets of
   routines, associated reference documents, a programming task designed to
   teach the use of the routines, and an example solution to the
   programming problem.
 
 
Overview
--------------------------------------------------------
 
   This workbook contains lessons to demonstrate use of the less celebrated
   Mice routines.
 
       1.   Kernel Management with the Kernel Subsystem
 
       2.   The Kernel Pool
 
       3.   Coordinate Conversions
 
       4.   Advanced Time Manipulation Routines
 
       5.   Error Handling
 
       6.   Windows and Cells
 
       7.   Utility and Constants Routines
 
 
Note About HTML Links
--------------------------------------------------------
 
   The HTML version of this lesson contains links pointing to various HTML
   documents provided with the Toolkit. All of these links are relative
   and, in order to function, require this document to be in a certain
   location in the Toolkit HTML documentation directory tree.
 
   In order for the links to be resolved, if not done already by installing
   the lessons package under the Toolkit's ``doc/html'' directory, create a
   subdirectory called ``lessons'' under the ``doc/html'' directory of the
   ``mice/'' tree and copy this document to that subdirectory before
   loading it into a Web browser.
 
 
References
--------------------------------------------------------
 
   This section lists SPICE documents referred to in this lesson.
 
   Of these documents, the ``Tutorials'' contains the highest level
   descriptions with the least number of details while the ``Required
   Reading'' documents contain much more detailed specifications. The most
   complete specifications are provided in the ``API Documentation''.
 
 
Tutorials
 
   The following SPICE tutorials serve as references for the discussions in
   this lesson:
 
 
      Name              Lesson steps/functions it describes
      ----------------  -----------------------------------------------
      concepts          Concepts of space geometry and time
      intro_to_kernels  Using kernels, meta-kernels
      time              Time systems, conversions and formats
      lsk_and_sclk      LSK and SCLK
      derived_quant     "high-level" observation geometry computations
      other_functions   Intro to some SPICE "low level" computations
      exceptions        built-in mechanism for trapping/handling errors
 
 
   These tutorials are available from the NAIF ftp server at JPL:
 
      http://naif.jpl.nasa.gov/naif/tutorials.html
 
 
Required Readings
 
   The Required Reading documents are provided with the Toolkit and are
   located under the ``mice/doc'' directory in the Mice installation tree.
 
      Name             Lesson steps/functions that it describes
      ---------------  -----------------------------------------
      kernel.req       Loading SPICE kernels
      time.req         Time conversion
      windows.req      The SPICE window data type
      mice.req         The Mice API
 
 
The Permuted Index
 
   Another useful document distributed with the Toolkit is the permuted
   index. This is located under the ``mice/doc'' directory in the MATLAB
   installation tree.
 
   This text document provides a simple mechanism by which users can
   discover which Mice functions perform functions of interest, as well as
   the names of the source files that contain these functions.
 
 
 
Mice API Documentation
 
   A Mice routine's specification is found in the HTML API documentation
   page located under ``mice/doc/html/mice''.
 
   For example, the document
 
      mice/doc/html/mice/cspice_str2et.html
 
   describes the cspice_str2et routine.
 
 
Kernels Used
--------------------------------------------------------
 
   The following kernels are used in examples provided in this lesson:
 
      #  FILE NAME    TYPE DESCRIPTION
      -- ------------ ---- ------------------------------------------------
      1  naif0008.tls LSK  Generic LSK
      2  de405s.bsp   SPK  Planet Ephemeris SPK
      3  pck00008.tpc PCK  Generic PCK
 
   These SPICE kernels are included in the lesson package available from
   the NAIF server at JPL:
 
      ftp://naif.jpl.nasa.gov/pub/naif/toolkit_docs/Lessons/
 
 
Mice Modules Used
--------------------------------------------------------
 
   This section provides a complete list of the functions and kernels that
   are suggested for usage in each of the exercises in this lesson. (You
   may wish to not look at this list unless/until you ``get stuck'' while
   working on your own.)
 
      CHAPTER EXERCISE   FUNCTIONS      NON-VOID       KERNELS
      ------- ---------  -------------  -------------  ----------
         1    kpool      cspice_furnsh  cspice_ktotal  1-3
                         cspice_unload  cspice_kdata
                         cspice_kclear
 
         2    kervar     cspice_furnsh  cspice_gnpool  1-3
                         cspice_kclear  cspice_dtpool
                                        cspice_gdpool
                                        cspice_gcpool
 
         3    coord      cspice_furnsh  cspice_str2et  1-3
                         cspice_kclear  cspice_bodvrd
                                        cspice_spkpos
                                        cspice_recrad
                                        cspice_dpr
                                        cspice_reclat
                                        cspice_recsph
                                        cspice_recgeo
 
         4    xtic       cspice_furnsh  cspice_str2et  1
                         cspice_tsetyr  cspice_timout
                         cspice_kclear  cspice_tpictr
                                        cspice_jyear
 
         5    aderr      cspice_furnsh  cspice_spkezr  1-3
                         cspice_kclear
 
         6    win        cspice_furnsh  cspice_str2et  1-3
                         cspice_kclear  cspice_wninsd
                                        cspice_wnvald
                                        cspice_wnintd
                                        cspice_wnfetd
                                        cspice_et2utc
                                        cspice_wnsumd
 
         7    units                     cspice_tkvrsn
                                        cspice_convrt
 
              xconst                    cspice_spd
                                        cspice_dpr
                                        cspice_rpd
                                        cspice_clight
                                        cspice_j2100
                                        cspice_j2000
                                        cspice_tyear
                                        cspice_halfpi
 
   Refer to the Mice HTML API documentation pages located under
   ``mice/doc/html/mice'' for detailed interface specifications of these
   functions.
 
 
NAIF Documentation
===========================================================================
 
   The technical complexity of the various SPICE subsystems mandates an
   extensive, user-friendly documentation set. The set differs somewhat
   depending on your choice of development language but provides the same
   information with regards to SPICE operation. The sources for a user
   needing information concerning SPICE are:
 
       --   Required Readings and Users Guides
 
       --   Library Source Code Documentation
 
       --   API Documentation
 
       --   Tutorials
 
 
Required Reading and Users Guides
 
   NAIF Required Reading (*.req) documents introduce the functionality of
   particular Mice subsystems:
 
      abcorr.req
      cells.req
      ck.req
      cspice.req
      daf.req
      das.req
      dla.req
      dsk.req
      ek.req
      ellipses.req
      error.req
      frames.req
      gf.req
      kernel.req
      mice.req
      naif_ids.req
      pck.req
      planes.req
      problems.req
      rotation.req
      scanning.req
      sclk.req
      sets.req
      spc.req
      spk.req
      symbols.req
      time.req
      windows.req
 
   NAIF Users Guides (*.ug) describe the proper use of particular Mice
   tools:
 
      brief.ug
      chronos.ug
      ckbrief.ug
      commnt.ug
      convert.ug
      dskbrief.ug
      dskexp.ug
      frmdiff.ug
      inspekt.ug
      mkdsk.ug
      mkspk.ug
      msopck.ug
      simple.ug
      spacit.ug
      spkdiff.ug
      spkmerge.ug
      states.ug
      subpt.ug
      tictoc.ug
      tobin.ug
      toxfr.ug
      version.ug
 
   These text documents exist in the 'doc' directory of the main Toolkit
   directory:
 
         ../mice/doc/
 
 
HTML format documentation
 
   The Mice distributions include HTML versions of Required Readings and
   Users Guides, accessible from the HTML documentation directory:
 
        ../mice/doc/html/index.html
 
 
Library Source Code Documentation
 
   All SPICELIB and CSPICE source files include usage and design
   information incorporated in a comment block known as the "header."
   (Every toolkit includes either the SPICELIB or CSPICE library.)
 
   A header consists of several marked sections:
 
       --   Procedure: Routine name and one line expansion of the routine's
            name.
 
       --   Abstract: A tersely worded explanation describing the routine.
 
       --   Copyright: An identification of the copyright holder for the
            routine.
 
       --   Required_Reading: A list of Mice required reading documents
            relating to the routine.
 
       --   Brief_I/O: A table of arguments, identifying each as either
            input, output, or both, with a very brief description of the
            variable.
 
       --   Detailed_Input & Detailed_Output: An elaboration of the
            Brief_I/O section providing comprehensive information on
            argument use.
 
       --   Parameters: Description and declaration of any parameters
            (constants) specific to the routine.
 
       --   Exceptions: A list of error conditions the routine detects and
            signals plus a discussion of any other exceptional conditions
            the routine may encounter.
 
       --   Files: A list of other files needed for the routine to operate.
 
       --   Particulars: A discussion of the routine's function (if
            needed). This section may also include information relating to
            "how" and "why" the routine performs an operation and to
            explain functionality of routines that operate by side effects.
 
       --   Examples: Descriptions and code snippets concerning usage of
            the routine.
 
       --   Restrictions: Restrictions or warnings concerning use.
 
       --   Literature_References: A list of sources required to understand
            the algorithms or data used in the routine.
 
       --   Author_and_Institution: The names and affiliations for authors
            of the routine.
 
       --   Version: A list of edits and the authors of those edits made to
            the routine since initial delivery to the Mice system.
 
   The source code for Mice products is stored in 'src' sub-directory of
   the main Mice directory:
 
         ../mice/src/
 
   Find the CSPICE library source code in:
 
         ../mice/src/cspice/
 
   Note: The CSPICE source files have two forms: C files created by the f2c
   conversion process on a SPICELIB files, indicated with a name of the
   form "module.c," and wrappers files indicated by names of the form
   "module_c.c" The f2c converted source code is very difficult to read,
   refer to the wrapper routines if possible. In some cases, NAIF replaced
   an f2c converted file with a hand written version.
 
 
API Documentation
 
   The Mice package includes the CSPICE Reference Guide, an index of all
   CSPICE wrapper APIs with hyperlinks to API specific documentation. Each
   API documentation page includes cross-links to any other wrapper API
   mentioned in the document and links to the wrapper source code.
 
         ...mice/doc/html/cspice/index.html
 
   Also included is Mice Reference Guide, an index of all Mice APIs with
   hyperlinks to API specific documentation. Each API documentation page
   includes cross-links to any other Mice APIs mentioned in the document
   and a link to the API documentation for the CSPICE routine called by the
   Mice interface.
 
         ...mice/doc/html/mice/index.html
 
   This Mice API documentation (the same information as in the Reference
   Guide but without hyperlinks) is also available from the Matlab "help"
   command:
 
      >> help cspice_illum
       -Abstract
 
          CSPICE_ILLUM calculates the illumination angles at a specified
          surface point of a target body.
 
                                      ...
 
 
Text kernels
--------------------------------------------------------
 
   Several workbooks use SPICE text kernels. SPICE identifies a text kernel
   as an ASCII text file containing the mark-up tags the kernel subsystem
   requires to identify data assignments in that file, and "name=value"
   data assignments.
 
   The subsystem uses two tags:
 
         \begintext
 
   and
 
         \begindata
 
   to mark information blocks within the text kernel. The \begintext tag
   specifies all text following the tag as comment information to be
   ignored by the subsystem.
 
   Things to know:
 
       1.   The \begindata tag marks the start of a data definition block.
            The subsystem processes all text following this marker as SPICE
            kernel data assignments until finding a \begintext marker.
 
       2.   The kernel subsystem defaults to the \begintext mode until the
            parser encounters a \begindata tag. Once in \begindata mode the
            subsystem processes all text as variable assignments until the
            next \begintext tag.
 
       3.   Enter the tags as the only text on a line, i.e.:
 
 
         \begintext
 
            ... commentary information on the data assignments ...
 
         \begindata
 
            ... data assignments ...
 
 
       4.   CSPICE delivery N0059 added to the CSPICE and Icy text kernel
            parsers the functionality to read non native text kernels, i.e.
            a Unix compiled library can read a MS Windows native text
            kernel, a MS Windows compiled library can read a Unix native
            text kernel. Mice acquires this capability from CSPICE.
 
       5.   With regards to the FORTRAN distribution, as of delivery N0057
            the cspice_furnsh call includes a line terminator check,
            signaling an error on any attempt to read non-native text
            kernels.
 
 
Text kernel format
 
   Scalar assignments.
 
         VAR_NAME_DP  = 1.234
         VAR_NAME_INT = 1234
         VAR_NAME_STR = 'FORBIN'
 
   Please note the use of a single quote in string assignments.
 
   Vector assignments. Vectors must contain the same type data.
 
         VEC_NAME_DP  = ( 1.234   , 45.678  , 901234.5 )
         VEC_NAME_INT = ( 1234    , 456     , 789      )
         VEC_NAME_STR = ( 'FORBIN', 'FALKEN', 'ROBUR'  )
 
         also
 
         VEC_NAME_DP  = ( 1.234,
                         45.678,
                         901234.5 )
 
         VEC_NAME_STR = ( 'FORBIN',
                          'FALKEN',
                          'ROBUR' )
 
   Time assignments.
 
         TIME_VAL = @31-JAN-2003-12:34:56.798
         TIME_VEC = ( @01-DEC-2004, @15-MAR-2004 )
 
   The at-sign character '@' indicates a time string. The pool subsystem
   converts the strings to double precision TDB (a numeric value). Please
   note, the time strings must not contain embedded blanks. WARNING - a TDB
   string is not the same as a UTC string.
 
   The above examples depict direct assignments via the '=' operator. The
   kernel pool also permits incremental assignments via the '+=' operator.
 
   Please refer to the kernels required reading, kernel.req, for additional
   information.
 
 
Lesson 1: Kernel Management with the Kernel Subsystem
===========================================================================
 
 
Task Statement
--------------------------------------------------------
 
   Write a program to load a meta kernel, interrogate the Mice system for
   the names and types of all loaded kernels, then demonstrate the unload
   functionality and the resulting effects.
 
 
Learning Goals
--------------------------------------------------------
 
   This lesson demonstrates use of the kernel subsystem to load, unload,
   and list loaded kernels.
 
   This lesson requires creation of a SPICE meta kernel.
 
 
Code Solution
--------------------------------------------------------
 
 
First, create a meta text kernel:
 
   You can use two versions of a meta kernel with code examples (kpool.tm)
   in this lesson. Either a kernel with explicit path information:
 
      KPL/MK
 
      \begindata
 
         KERNELS_TO_LOAD = ( 'kernels/spk/de405s.bsp',
                             'kernels/pck/pck00008.tpc',
                             'kernels/lsk/naif0008.tls' )
 
      \begintext
 
   ... or a more generic meta kernel using the PATH_VALUES/PATH_SYMBOLS
   functionality to declare path names as variables:
 
      KPL/MK
 
         Define the paths to the kernel directory. Use the PATH_SYMBOLS
         as aliases to the paths.
 
         The names and contents of the kernels referenced by this
         meta-kernel are as follows:
 
            File Name        Description
            ---------------  ------------------------------
            naif0008.tls     Generic LSK.
            de405s.bsp       Planet Ephemeris SPK.
            pck00008.tpc     Generic PCK.
 
 
      \begindata
 
         PATH_VALUES     = ( 'kernels/lsk',
                             'kernels/spk',
                             'kernels/pck' )
 
         PATH_SYMBOLS    = ( 'LSK', 'SPK', 'PCK' )
 
         KERNELS_TO_LOAD = ( '$LSK/naif0008.tls',
                             '$SPK/de405s.bsp',
                             '$PCK/pck00008.tpc' )
 
      \begintext
 
 
Now the solution source code:
 
      function kpool()
 
         %
         % Assign the path name of the meta kernel to META.
         %
         META = 'kpool.tm';
 
         %
         % Load the meta kernel then use KTOTAL to interrogate the SPICE
         % kernel subsystem.
         %
         cspice_furnsh( META )
 
         count = cspice_ktotal( 'ALL' );
         fprintf( 'Kernel count after load:        %i\n', count )
 
 
         %
         % Loop over the number of files; interrogate the SPICE system
         % with kdata_c for the kernel names and the type. 'found'
         % returns a boolean indicating whether any kernel files of
         % the specified type were loaded by the kernel subsystem.
         % This example ignores checking 'found' as kernels are known
         % to be loaded.
         %
         for i = 1:count
            [ file, type, source, handle, found] = cspice_kdata(i, 'ALL');
            fprintf( 'File   %s\n', file )
            fprintf( 'Type   %s\n', type )
            fprintf( 'Source %s\n\n', source )
         end
 
         %
         % Unload one kernel then check the count.
         %
         cspice_unload( 'kernels/spk/de405s.bsp')
         count = cspice_ktotal( 'ALL' );
 
         %
         % The subsystem should report one less kernel.
         %
         fprintf( 'Kernel count after one unload:  %i\n', count )
 
         %
         % Now unload the meta kernel. This action unloads all
         % files listed in the meta kernel.
         %
         cspice_unload( META )
 
 
         %
         % Check the count. Icy should return a count of zero.
         %
         count = cspice_ktotal( 'ALL');
         fprintf( 'Kernel count after meta unload: %i\n', count )
 
         %
         % Done. Unload the kernels.
         %
         cspice_kclear
 
 
Run the code example
 
   First we see the number of all loaded kernels returned from the
   cspice_ktotal call.
 
   Then the cspice_kdata loop returns the name of each loaded kernel, the
   type of kernel (SPK, CK, TEXT, etc.) and the source of the kernel - the
   mechanism that loaded the kernel. The source either identifies a meta
   kernel, or contains an empty string. An empty source string indicates a
   direct load of the kernel with a cspice_furnsh call.
 
      Kernel count after load:        4
      File   kpool.tm
      Type   META
      Source
 
      File   kernels/lsk/naif0008.tls
      Type   TEXT
      Source kpool.tm
 
      File   kernels/spk/de405s.bsp
      Type   SPK
      Source kpool.tm
 
      File   kernels/pck/pck00008.tpc
      Type   TEXT
      Source kpool.tm
 
      Kernel count after one unload:  3
      Kernel count after meta unload: 0
 
 
Lesson 2: The Kernel Pool
===========================================================================
 
 
Task Statement
--------------------------------------------------------
 
   Write a program to retrieve particular string and numeric text kernel
   variables, both scalars and arrays. Interrogate the kernel pool for
   assigned variable names.
 
 
Learning Goals
--------------------------------------------------------
 
   The lesson demonstrates the Mice system's facility to retrieve different
   types of data (string, numeric, scalar, array) from the kernel pool.
 
   For the code examples, use this generic text kernel (kervar.tm)
   containing PCK-type data, kernels to load, and example time strings:
 
      KPL/MK
 
         Name the kernels to load. Use path symbols.
 
         The names and contents of the kernels referenced by this
         meta-kernel are as follows:
 
            File Name        Description
            ---------------  ------------------------------
            naif0008.tls     Generic LSK.
            de405s.bsp       Planet Ephemeris SPK.
            pck00008.tpc     Generic PCK.
 
 
      \begindata
 
         PATH_VALUES     = ('kernels/spk',
                            'kernels/pck',
                            'kernels/lsk')
 
         PATH_SYMBOLS    = ('SPK' , 'PCK' , 'LSK' )
 
         KERNELS_TO_LOAD = ( '$SPK/de405s.bsp',
                             '$PCK/pck00008.tpc',
                             '$LSK/naif0008.tls')
 
      \begintext
 
      Ring model data.
 
      \begindata
 
         BODY699_RING1_NAME     = 'A Ring'
         BODY699_RING1          = (122170.0 136780.0 0.1 0.1 0.5)
 
         BODY699_RING1_1_NAME   = 'Encke Gap'
         BODY699_RING1_1        = (133405.0 133730.0 0.0 0.0 0.0)
 
         BODY699_RING2_NAME     = 'Cassini Division'
         BODY699_RING2          = (117580.0 122170.0 0.0 0.0 0.0)
 
      \begintext
 
      The kernel pool recognizes values preceded by '@' as time
      values. When read, the kernel subsystem converts these
      representations into double precision ephemeris time.
 
      Caution: The kernel subsystem interprets the time strings
      identified by '@' as TDB. The same string passed as input
      to @STR2ET is processed as UTC.
 
      The three expressions stored in the EXAMPLE_TIMES array represent
      the same epoch.
 
      \begindata
 
         EXAMPLE_TIMES       = ( @APRIL-1-2004-12:34:56.789,
                                 @4/1/2004-12:34:56.789,
                                 @JD2453097.0242684
                                )
 
      \begintext
 
 
   The main references for pool routines are found in the help command or
   API documentation for the particular routines.
 
 
Code Solution
--------------------------------------------------------
 
      function kervar()
 
         %
         % Define the max number of kernel variables
         % of concern for this examples.
         %
         N_ITEMS =  20;
 
         %
         % Load the example kernel containing the kernel variables.
         % The kernels defined in KERNELS_TO_LOAD load into the
         % kernel pool with this call.
         %
         cspice_furnsh( 'kervar.tm' )
 
         %
         % Initialize the start value. This values indicates
         % index of the first element to return if a kernel
         % variable is an array. START = 1 indicates return everything.
         % START = 2 indicates return everything but the first element.
         %
         START = 1;
 
         %
         % Set the template for the variable names to find. Let's
         % look for all variables containing  the string RING.
         % Define this with the wildcard template '*RING*'. Note:
         % the template '*RING' would match any variable name
         % ending with the RING string.
         %
         tmplate = '*RING*';
 
         %
         % We're ready to interrogate the kernel pool for the
         % variables matching the template. cspice_gnpool tells us:
         %
         %  1. Does the kernel pool contain any variables that
         %     match the template (value of found).
         %  2. If so, how many variables?
         %  3. The variable names. (cvals, an array of strings)
         %
 
         [cvals,found] = cspice_gnpool( tmplate, START, N_ITEMS );
 
         if ( found )
            fprintf( 'Number variables matching template: %i\n\n', ...
                                                   size(cvals,1) )
         else
            disp( 'No kernel variables matched template.\n\n' )
         return
         end
 
         %
         % For convenience, convert the character array to a cell of
         % strings.
         %
         cvals = cellstr( cvals );
 
         %
         % Okay, now we know something about the kernel pool
         % variables of interest to us. Let's find out more...
         %
         for i=1:size(cvals,1)
 
            %
            % Use cspice_dtpool to return the dimension and type,
            % C (character) or N (numeric), of each pool
            % variable name in the cvals array. We know 'found'
            % will have value true.
            %
            [found, dim, type] = cspice_dtpool( cvals(i) );
 
            disp( cvals(i) )
            fprintf( ' Number items: %i   Of type: %s\n', dim, type );
 
            %
            % Test character equality, 'N' or 'C'.
            %
            switch type
 
               case 'N'
 
                  %
                  % If 'type' equals 'N', we found a numeric array.
                  % In this case any numeric array will be an array
                  % of double precision numbers ('doubles').
                  % cspice_gdpool retrieves doubles from the
                  % kernel pool.
                  %
                  [dvars,found] = cspice_gdpool( cvals(i), ...
                                                 START,    ...
                                                 N_ITEMS );
                  fprintf('  Numeric value: %20.6f\n', dvars )
 
               case 'C'
 
                  %
                  % If 'type' equals 'C', we found a string array.
                  % cspice_gcpool retrieves string values from the
                  % kernel pool.
                  %
                  [cvars,found] = cspice_gcpool( cvals(i), ...
                                                 START,    ...
                                                 N_ITEMS );
 
                  for j=1:size(cvars,1)
 
                     fprintf('  String value: %s\n', cvars(j,:) )
 
                  end
 
            end
 
            disp(' ')
 
         end
 
 
         %
         % Now look at the time variable EXAMPLE_TIMES. Extract this
         % value as an array of doubles.
         %
         [dvars,found] = cspice_gdpool( 'EXAMPLE_TIMES', START, N_ITEMS );
 
         disp( 'EXAMPLE_TIMES' )
         fprintf('  Time value:    %20.6f\n', dvars)
 
         %
         % Done. Unload the kernels.
         %
         cspice_kclear
 
 
Run the code example
 
   The program runs and first reports the number of kernel pool variables
   matching the template, 6.
 
   The program then loops over the cspice_dtpool 6 times, reporting the
   name of each pool variable, the number of data items assigned to that
   variable, and the variable type. Within the cspice_dtpool loop, a second
   loop outputs the contents of the data variable using cspice_gcpool or
   cspice_gdpool.
 
      Number variables matching template: 6
 
          'BODY699_RING1_1'
 
       Number items: 5   Of type: N
        Numeric value:        133405.000000
        Numeric value:        133730.000000
        Numeric value:             0.000000
        Numeric value:             0.000000
        Numeric value:             0.000000
 
          'BODY699_RING1'
 
       Number items: 5   Of type: N
        Numeric value:        122170.000000
        Numeric value:        136780.000000
        Numeric value:             0.100000
        Numeric value:             0.100000
        Numeric value:             0.500000
 
          'BODY699_RING2'
 
       Number items: 5   Of type: N
        Numeric value:        117580.000000
        Numeric value:        122170.000000
        Numeric value:             0.000000
        Numeric value:             0.000000
        Numeric value:             0.000000
 
          'BODY699_RING1_1_NAME'
 
       Number items: 1   Of type: C
        String value: Encke Gap
 
          'BODY699_RING2_NAME'
 
       Number items: 1   Of type: C
        String value: Cassini Division
 
          'BODY699_RING1_NAME'
 
       Number items: 1   Of type: C
        String value: A Ring
 
      EXAMPLE_TIMES
        Time value:        134094896.789000
        Time value:        134094896.789000
        Time value:        134094896.789753
 
   Note the final time value differs from the previous values in the final
   three decimal places despite the intention that all three strings
   represent the same time. This results from round-off when converting a
   decimal Julian day representation to the seconds past J2000 ET
   representation.
 
 
Related Routines
--------------------------------------------------------
 
       --   cspice_gipool retrieves integer values from the kernel
            subsystem.
 
 
Lesson 3: Coordinate Conversions
===========================================================================
 
 
Task Statement
--------------------------------------------------------
 
   Write a program to convert a Cartesian 3-vector representing some
   location to the other coordinate representations. Use the position of
   the Moon with respect to Earth in an inertial and non-inertial reference
   frame as the example vector.
 
 
Learning Goals
--------------------------------------------------------
 
   The Mice system provides functions to convert coordinate tuples between
   Cartesian and various non Cartesian coordinate systems including
   conversion between geodetic and rectangular coordinates.
 
   This lesson presents these coordinate transform routines for
   rectangular, cylindrical, and spherical systems.
 
 
Code Solution
--------------------------------------------------------
 
      function coord()
 
         %
         % Define the inertial and non inertial frame names.
         %
         % Initialize variables or set type. All variables
         % used in a PROMPT construct must be initialized
         % as strings.
         %
         INRFRM = 'J2000';
         NONFRM = 'IAU_EARTH';
 
         %
         % Load the needed kernels using a cspice_furnsh call on the
         % meta kernel.
         %
         cspice_furnsh( 'coord.tm' )
 
         %
         % Prompt the user for a time string. Convert the
         % time string to ephemeris time J2000 (ET).
         %
         timstr = input( 'Time of interest: ', 's' );
         et     = cspice_str2et( timstr );
 
         %
         % Access the kernel pool data for the triaxial radii of the
         % Earth, rad[0] holds the equatorial radius, rad[2]
         % the polar radius.
         %
         rad = cspice_bodvrd( 'EARTH', 'RADII', 3 );
 
         %
         % Calculate the flattening factor for the Earth.
         %
         %          equatorial_radius - polar_radius
         % flat =   ________________________________
         %
         %                equatorial_radius
         %
         flat = (rad(1) - rad(3))/rad(1);
 
         %
         % Make the cspice_spkpos call to determine the apparent
         % position of the Moon w.r.t. to the Earth at 'et' in the
         % inertial frame.
         %
         [pos, ltime] = cspice_spkpos('MOON', et, INRFRM, 'LT+S','EARTH');
 
         %
         % Show the current frame and time.
         %
         disp( [' Time : ' timstr ] )
         disp( [' Inertial Frame: ' INRFRM  ] )
 
         %
         % First convert the position vector
         % X = pos(1), Y = pos(2), Z = pos(3), to RA/DEC.
         %
         [ range, ra, dec ] = cspice_recrad( pos );
         disp('   Range/Ra/Dec' )
         fprintf('    Range: %20.6f\n', range )
         fprintf('    RA   : %20.6f\n',  ra * cspice_dpr )
         fprintf('    DEC  : %20.6f\n', dec * cspice_dpr )
 
         %
         % ...latitudinal coordinates...
         %
         [ range, lon, lat ] = cspice_reclat( pos );
         disp('   Latitudinal ' )
         fprintf('    Rad  : %20.6f\n', range )
         fprintf('    Lon  : %20.6f\n', lon * cspice_dpr )
         fprintf('    Lat  : %20.6f\n', lat * cspice_dpr )
 
         %
         % ...spherical coordinates use the colatitude,
         % the angle from the Z axis.
         %
         [ range, colat, lon ] = cspice_recsph( pos );
         disp( '   Spherical' )
         fprintf('    Rad  : %20.6f\n', range )
         fprintf('    Lon  : %20.6f\n', lon   * cspice_dpr )
         fprintf('    Colat: %20.6f\n', colat * cspice_dpr )
 
         %
         % Make the cspice_spkpos call to determine the apparent
         % position of the Moon w.r.t. to the Earth at 'et' in the
         % non-inertial, body fixed, frame.
         %
         [pos, ltime] = cspice_spkpos('MOON', et, NONFRM, 'LT+S','EARTH');
 
         disp( ['  Non-inertial Frame: ' NONFRM ] )
 
         %
         % ...latitudinal coordinates...
         %
         [ range, lon, lat ] = cspice_reclat( pos );
         disp('   Latitudinal ' )
         fprintf('    Rad  : %20.6f\n', range )
         fprintf('    Lon  : %20.6f\n', lon * cspice_dpr )
         fprintf('    Lat  : %20.6f\n', lat * cspice_dpr )
 
         %
         % ...spherical coordinates use the colatitude,
         % the angle from the Z axis.
         %
         [ range, colat, lon ] = cspice_recsph( pos );
         disp( '   Spherical' )
         fprintf('    Rad  : %20.6f\n', range )
         fprintf('    Lon  : %20.6f\n', lon   * cspice_dpr )
         fprintf('    Colat: %20.6f\n', colat * cspice_dpr )
 
         %
         % ...finally, convert the position to geodetic coordinates.
         %
         [ lon, lat, range ] = cspice_recgeo( pos, rad(1), flat );
         disp( '   Geodetic' )
         fprintf('    Rad  : %20.6f\n', range )
         fprintf('    Lon  : %20.6f\n', lon * cspice_dpr )
         fprintf('    Lat  : %20.6f\n', lat * cspice_dpr )
 
         %
         % Done. Unload the kernels.
         %
         cspice_kclear
 
 
Run the code example
 
   Input "Feb 3 2002 TDB" to calculate the Moon's position. (the 'TDB' tag
   indicates a Barycentric Dynamical Time value).
 
      Time of interest: Feb 3 2002 TDB
 
   Examine the Moon position in the J2000 inertial frame, display the time
   and frame:
 
       Time : Feb 3 2002 TDB
        Inertial Frame: J2000
 
   Convert the Moon Cartesian coordinates to right ascension declination.
 
         Range/Ra/Dec
          Range:        369340.815193
          RA   :           203.643686
          DEC  :            -4.979010
 
   Latitudinal. Note the difference in the expressions for longitude and
   right ascension though they represent a measure of the same quantity.
   The RA/DEC system measures RA in the interval [0,2Pi). Latitudinal
   coordinates measures longitude in the interval (-Pi,Pi].
 
         Latitudinal
          Rad  :        369340.815193
          Lon  :          -156.356314
          Lat  :            -4.979010
 
   Spherical. Note the difference between the expression of latitude in the
   Latitudinal system and the corresponding Spherical colatitude. The
   spherical coordinate system uses the colatitude, the angle measure away
   from the positive Z axis. Latitude is the angle between the position
   vector and the x-y (equatorial) plane with positive angle defined as
   toward the positive Z direction
 
         Spherical
          Rad  :        369340.815193
          Lon  :          -156.356314
          Colat:            94.979010
 
   The same position look-up in a body fixed (non-inertial) frame,
   IAU_EARTH.
 
 
        Non-inertial Frame: IAU_EARTH
 
   Latitudinal coordinates return the geocentric latitude.
 
         Latitudinal
          Rad  :        369340.815193
          Lon  :            70.986950
          Lat  :            -4.989675
 
   Spherical.
 
         Spherical
          Rad  :        369340.815193
          Lon  :            70.986950
          Colat:            94.989675
 
   Geodetic. The cartographic lat/lon.
 
         Geodetic
          Rad  :        362962.836755
          Lon  :            70.986950
          Lat  :            -4.990249
 
 
Related Routines
--------------------------------------------------------
 
       --   cspice_latrec, latitudinal to rectangular
 
       --   cspice_latcyl, latitudinal to cylindrical
 
       --   cspice_latsph, latitudinal to spherical
 
       --   cspice_reccyl, rectangular to cylindrical
 
       --   cspice_sphrec, spherical to rectangular
 
       --   cspice_sphcyl, spherical to cylindrical
 
       --   cspice_sphlat, spherical to latitudinal
 
       --   cspice_cyllat, cylindrical to latitudinal
 
       --   cspice_cylsph, cylindrical to spherical
 
       --   cspice_cylrec, cylindrical to rectangular
 
       --   cspice_georec, geodetic to rectangular
 
 
Lesson 4: Advanced Time Manipulation Routines
===========================================================================
 
 
Task Statement
--------------------------------------------------------
 
   Demonstrate the advanced functions of the time utilities with regard to
   formatting of time strings for output. Formatting options include
   altering calendar representations of the time strings. Convert time-date
   strings between different Mice-supported formats.
 
 
Learning Goals
--------------------------------------------------------
 
   Introduce the routines used for advanced manipulation of time strings.
   Understand the concept of ephemeris time (ET) as used in Mice.
 
 
Code Solution
--------------------------------------------------------
 
   Caution: Be sure to assign sufficient string lengths for time
   formats/pictures.
 
      function xtic()
 
         %
         % Assign the META variable to the name of the meta-kernel
         % that contains the LSK kernel and create an arbitrary
         % time string.
         %
         % Define the maximum length for any string, 80
         % characters plus one null terminator for C.
         %
         CALSTR    = 'Mar 15, 2003 12:34:56.789 AM PST';
         META      = 'xtic.tm';
         AMBIGSTR  = 'Mar 15, 79 12:34:56';
         T_FORMAT1 = 'Wkd Mon DD HR:MN:SC PDT YYYY ::UTC-7';
         T_FORMAT2 = 'Wkd Mon DD HR:MN ::UTC-7 YR (JULIAND.##### JDUTC)';
 
         %
         % Load the meta-kernel.
         %
         cspice_furnsh( META )
         disp( [ 'Original time string     : ' CALSTR ] )
 
         %
         % Convert the time string to the number of ephemeris
         % seconds past the J2000 epoch. This is the most common
         % internal time representation used by the CSPICE
         % system; CSPICE refers to this as ephemeris time (ET).
         %
         et = cspice_str2et( CALSTR );
         fprintf( 'Corresponding ET         : %20.6f\n', et )
 
         %
         % Make a picture of an output format. Describe a Unix-like
         % time string then send the picture and the 'et' value through
         % cspice_timout to format and convert the ET representation
         % of the time string into the form described in cspice_timout.
         % The '::UTC-7' token indicates the time zone for the 'timstr'
         % output - PDT. 'PDT' is part of the output, but not a time
         % system token.
         %
         timstr = cspice_timout( et, T_FORMAT1);
         fprintf( 'Time in string format 1  : %s\n', timstr )
 
         timstr = cspice_timout( et, T_FORMAT2);
         fprintf( 'Time in string format 2  : %s\n', timstr )
 
         %
         % Why create a picture by hand when Mice can do it for you?
         % Input a string to cspice_tpictr with the format of interest.
         % 'ok' returns a boolean indicating whether an error occurred
         % while parsing the picture string, if so, an error diagnostic
         % message returns in 'xerror'. In this example the picture
         % string is known as correct.
         %
         pic = '12:34:56.789 P.M. PDT January 1, 2006';
         [ pictr, ok, xerror] = cspice_tpictr(pic);
 
         if ( ~ok )
            error( xerror )
         end
 
         timstr = cspice_timout( et, pictr);
         fprintf( 'Time in string format 3  : %s\n', timstr )
 
         %
         % Two digit year representations often cause problems due to
         % the ambiguity of the century. The routine cspice_tsetyr gives
         % the user the ability to set a default range for 2 digit year
         % representation. SPICE uses 1969AD as the default start
         % year so the numbers inclusive of 69 to 99 represent years
         % 1969AD to 1999AD, the numbers inclusive of 00 to 68 represent
         % years 2000AD to 2068AD.
         %
         % The defined time string 'AMBIGSTR' contains a two-digit
         % year. Since the SPICE base year is 1969, the time subsystem
         % interprets the string as 1979.
         %
         et1 = cspice_str2et( AMBIGSTR );
 
         %
         % Set 1980 as the base year causes SPICE to interpret the
         % time string's "79" as 2079.
         %
         cspice_tsetyr( 1980 )
         et2 = cspice_str2et( AMBIGSTR );
 
         %
         % Calculate the number of years between the two ET
         % representations, ~100.
         %
         fprintf( 'Years between evaluations:  %20.6f\n', ...
                                     (et2 - et1)/cspice_jyear )
 
         %
         % Reset the default year to 1969.
         %
         cspice_tsetyr( 1969 )
 
         %
         % Done. Unload the kernels.
         %
         cspice_kclear
 
 
Run the code example
 
      Original time string     : Mar 15, 2003 12:34:56.789 AM PST
      Corresponding ET         :     100989360.974561
      Time in string format 1  : Sat Mar 15 01:34:56 PDT 2003
      Time in string format 2  : Sat Mar 15 01:34  03 (2452713.85760 JDUTC)
      Time in string format 3  : 01:34:56.789 A.M. PDT March 15, 2003
      Years between evaluations:            100.000000
 
 
Lesson 5: Error Handling
===========================================================================
 
 
Task Statement
--------------------------------------------------------
 
   Write an interactive program to return a state vector based on a user's
   input. Code the program with the capability to recover from user input
   mistakes, inform the user of the mistake, then continue to run.
 
 
Learning Goals
--------------------------------------------------------
 
   Learn how to write a program that has the capability to recover from
   expected SPICE errors.
 
   The Mice error subsystem differs from CSPICE and SPICELIB packages in
   that the user cannot alter the state of the error subsystem, rather the
   user can respond to an error signal using try-catch blocks. This block
   natively receives and processes any SPICE error signaled from Mice. The
   user can therefore "catch" an error signal so as to respond in an
   appropriate manner.
 
 
Code Solution
--------------------------------------------------------
 
      function aderr()
 
         %
         % Set initial parameters.
         %
         SPICETRUE =  logical(1);
         SPICEFALSE=  logical(0);
         doloop    =  SPICETRUE;
 
         %
         % Load the data we need for state evaluation.
         %
         cspice_furnsh( 'aderr.tm' )
 
         %
         % Start our input query loop to the user.
         %
         while (doloop)
 
            %
            % For simplicity, we request only one input.
            % The program calculates the state vector from
            % Earth to the user specified target 'targ' in the
            % J2000 frame, at ephemeris time zero, using
            % aberration correction LT+S (light time plus
            % stellar aberration).
            %
            targ = input( 'Target: ', 's' );
 
            if ( strcmpi( targ, 'NONE') )
 
               %
               % An exit condition. If the user inputs NONE
               % for a target name, set the loop to stop...
               %
               doloop = SPICEFALSE;
 
            else
 
               %
               % ...otherwise evaluate the state between the Earth
               % and the target. Initialize an error handler.
               %
               try
 
                  %
                  % Perform the state lookup.
                  %
                  [ state, ltime] = cspice_spkezr( targ, 0., 'J2000', ...
                                                             'LT+S' , ...
                                                             'EARTH');
 
                  %
                  % No error, output the state.
                  %
                  fprintf( 'R : %20.6f %20.6f %20.6f\n', state(1:3)' )
                  fprintf( 'V : %20.6f %20.6f %20.6f\n', state(4:6)' )
                  fprintf( 'LT: %20.6f\n\n', ltime )
 
               catch
 
                  %
                  % What if cspice_spkezr signaled an error?
                  % Then Mice signals an error to MATLAB.
                  %
                  % Examine the value of 'lasterr' to retrieve the
                  % error message.
                  %
                  disp( lasterr )
                  disp(' ')
 
              end
 
            end
 
         end
 
         %
         % Done. Unload the kernels.
         %
         cspice_kclear
 
 
Run the code example
 
   Now run the code with various inputs to observe behavior. Begin the run
   using known astronomical bodies, e.g. "Moon", "Mars", "Pluto barycenter"
   and "Puck". Recall the Mice default units are kilometers, kilometers per
   second, kilograms, and seconds. The 'R' marker identifies the (X,Y,Z)
   position of the body in kilometers, the 'V' marker identifies the
   velocity of the body in kilometers per second, and the 'LT' marker
   identifies the one-way light time between the bodies at the requested
   evaluation time.
 
      Target: Moon
      R :       -291584.616595       -266693.402359        -76095.647558
      V :             0.643439            -0.666066            -0.301310
      LT:             1.342311
 
      Target: Mars
      R :     234536077.419136    -132584383.595569     -63102685.706191
      V :            30.961373            28.932996            13.113031
      LT:           923.001080
 
      Target: Pluto barycenter
      R :   -1451304742.838526   -4318174144.406321    -918251433.587357
      V :            35.079843             3.053138            -0.036762
      LT:         15501.258293
 
      Target: Puck
      Error using mice
      SPICE(SPKINSUFFDATA): [spkezr_c->SPKEZR->SPKEZ->SPKACS->SPKAPS->SPKLT
      C->SPKGEO] Insufficient ephemeris data has been loaded to compute the
       state of 715 (PUCK) relative to 0 (SOLAR SYSTEM BARYCENTER) at the e
      phemeris epoch 2000 JAN 01 12:00:00.000.
 
      Target:
 
   Perplexing. What happened?
 
   The kernel files named in meta.tm did not include ephemeris data for
   Puck. When the SPK subsystem tried to evaluate Puck's position, the
   evaluation failed due to lack of data, so an error signaled.
 
   The above error signifies an absence of state information at ephemeris
   time 2000 JAN 01 12:00:00.000 (the requested time, ephemeris time zero).
 
   Try another look-up, this time for "Casper"
 
      Target: Casper
      Error using mice
      SPICE(IDCODENOTFOUND): [spkezr_c->SPKEZR] The target, 'Casper', is no
      t a recognized name for an ephemeris object. The cause of this proble
      m may be that you need an updated version of the SPICE Toolkit. Alter
      natively you may call SPKEZ directly if you know the SPICE ID codes f
      or both 'Casper' and 'EARTH'
 
      Target:
 
   An easy to understand error. The SPICE system does not contain
   information on a body named 'Casper.'
 
   Another look-up, this time, "Venus".
 
      Target: Venus
      R :     -80970027.540532    -139655772.573898     -53860125.958201
      V :            31.166910           -27.001056           -12.316514
      LT:           567.655074
 
      Target:
 
   The look-up succeeded despite two errors in our run. The Mice system can
   respond to error conditions (not system errors) in much the same fashion
   as languages with catch/throw instructions.
 
 
Lesson 6: Windows, and Cells
===========================================================================
 
 
Programming task
--------------------------------------------------------
 
   Given the times of line-of-sight for a vehicle from a ground station and
   the times for an acceptable Sun-station-vehicle phase angle, write a
   program to determine the time intervals common to both configurations.
 
 
Learning Goals
--------------------------------------------------------
 
   This lesson introduces the concepts of the SPICE data type 'window'.
 
   The Mice implementation of a SPICE windows consists of double precision
   Nx1 arrays with N an even or zero value.
 
   A 'window' is a type of cell containing ordered, double precision values
   describing a collection of zero or more intervals.
 
   We define an interval, 'i', as all double precision values bounded by
   and including an ordered pair of numbers,
 
         [ a , b ]
            i   i
 
   where
 
         a    <   b
          i   -    i
 
   The intervals within a window are both ordered and disjoint. That is,
   the beginning of each interval is greater than the end of the previous
   interval:
 
         b  <  a
          i     i+1
 
   A common use of the windows facility is to calculate the intersection
   set of a number of time intervals.
 
 
Code Solution
--------------------------------------------------------
 
      function win
 
         %
         % The windows hold 8 data, i.e. values four intervals.
         %
         MAXSIZ = 8;
 
         %
         % Define a set of time intervals. For the purposes of this
         % tutorial program, define time intervals representing
         % an unobscured line of sight between a ground station
         % and some body.
         %
         los = { 'Jan 1, 2003 22:15:02', 'Jan 2, 2003  4:43:29',  ...
                 'Jan 4, 2003  9:55:30', 'Jan 4, 2003 11:26:52',  ...
                 'Jan 5, 2003 11:09:17', 'Jan 5, 2003 13:00:41',  ...
                 'Jan 6, 2003 00:08:13', 'Jan 6, 2003  2:18:01' };
 
         %
         % A second set of intervals representing the times for which
         % an acceptable phase angle exits between the ground station,
         % the body and the Sun.
         %
         phase = { 'Jan 2, 2003 00:03:30', 'Jan 2, 2003 19:00:00', ...
                   'Jan 3, 2003  8:00:00', 'Jan 3, 2003  9:50:00', ...
                   'Jan 5, 2003 12:00:00', 'Jan 5, 2003 12:45:00', ...
                   'Jan 6, 2003 00:30:00', 'Jan 6, 2003 23:00:00' };
 
         %
         % Load our meta kernel for the leapseconds data.
         %
         cspice_furnsh( 'win.tm' )
 
         %
         % SPICE windows consist of double precision values; convert
         % the string time tags defined in the 'los'and 'phase'
         % arrays to double precision ET. Store the double values
         % in the 'loswin' and 'phswin' windows.
         %
         los_et = cspice_str2et( los   );
         phs_et = cspice_str2et( phase );
 
         %
         % Initialize the windows with the 'los_et' and 'phs_et'
         % values.
         %
         % Create two empty windows.
         %
         loswin = zeros(0,1);
         phswin = zeros(0,1);
 
         %
         % Mice windows lack a constant size as the windows interfaces
         % dynamically adjust window size before return, therefore the
         % SPICE concept of window cardinality degenerates to window size.
         %
         for i=1:(MAXSIZ/2)
            loswin = cspice_wninsd( los_et(2*i - 1), los_et(2*i), loswin );
            phswin = cspice_wninsd( phs_et(2*i - 1), phs_et(2*i), phswin );
         end
 
         %
         % Validate the cells as windows.
         %
         cspice_wnvald( loswin );
         cspice_wnvald( phswin );
 
         %
         % The issue for consideration, at what times do line of
         % sight events coincide with acceptable phase angles?
         % Perform the set operation AND on loswin, phswin,
         % (the intersection of the time intervals)
         % place the results in the window 'sched'.
         %
         sched = cspice_wnintd( loswin, phswin);
 
         %
         % Output the results. The number of intervals in 'sched'
         % is half the number of data points (the cardinality).
         %
         card = numel(sched);
 
         fprintf( 'No. data values in sched           : %2i\n', card )
 
         fprintf( 'Time intervals meeting defined criterion.\n' )
 
         for i=1:(card/2)
 
            %
            % Extract from the derived 'sched' the values defining the
            % time intervals.
            %
            [left, right ] = cspice_wnfetd( sched, i );
 
            %
            % Convert the ET values to UTC for human comprehension.
            %
            utcstr_l = cspice_et2utc( left , 'C', 3 );
            utcstr_r = cspice_et2utc( right, 'C', 3 );
 
            %
            % Output the UTC string and the corresponding index
            % for the interval.
            %
            fprintf( '%2i  %s   %s\n', i, utcstr_l, utcstr_r )
 
         end
 
         %
         % Summarize the 'sched' window.
         %
         [meas, avg, stddev, small, large] = cspice_wnsumd(sched);
 
         fprintf( '\nSummary of sched window\n\n' )
 
         fprintf( 'o Total measure of sched    : %16.6f\n', meas  )
         fprintf( 'o Average measure of sched  : %16.6f\n', avg   )
         fprintf( 'o Standard deviation of \n' )
         fprintf( '  the measures in sched     : %16.6f\n', stddev)
 
         %
         % The values for small and large refer to the indexes of the
         % values in the window ('sched'). The shortest interval is
         %
         %      [ sched.base[ sched.data + small]
         %        sched.base[ sched.data + small +1]  ];
         %
         % the longest is
         %
         %      [ sched.base[ sched.data + large]
         %        sched.base[ sched.data + large +1]  ];
         %
         % Output the interval indexes for the shortest and longest
         % intervals.
         %
         fprintf( 'o Index of shortest interval: %2d\n', (small+1)/2 )
         fprintf( 'o Index of longest interval : %2d\n', (large+1)/2 )
 
         %
         % Done. Unload the kernels.
         %
         cspice_kclear
 
 
   List the time intervals for which a line of sight exists during the time
   of a proper phase angle.
 
 
Run the code example
 
   The output window has the name `sched' (schedule).
 
   Output the amount of data held in `sched'.
 
      No. data values in sched           :  6
 
   List the time intervals for which a line of sight exists during the time
   of a proper phase angle.
 
      Time intervals meeting defined criterion.
       1  2003 JAN 02 00:03:30.000   2003 JAN 02 04:43:29.000
       2  2003 JAN 05 12:00:00.000   2003 JAN 05 12:45:00.000
       3  2003 JAN 06 00:30:00.000   2003 JAN 06 02:18:01.000
 
   Finally, an analysis of the `sched' data. The measure of an interval
   [a,b] (a <= b) equals b-a. Real values output in units of seconds.
 
 
      Summary of sched window
 
      o Total measure of sched    :     25980.000009
      o Average measure of sched  :      8660.000003
      o Standard deviation of
        the measures in sched     :      5958.550217
      o Index of shortest interval:  2
      o Index of longest interval :  1
 
 
Related Routines
--------------------------------------------------------
 
       --   cspice_wncomd determines the compliment of a window with
            respect to a defined interval.
 
       --   cspice_wncond contracts a window's intervals.
 
       --   cspice_wndifd : Calculate the difference between two windows;
            i.e. every point existing in the first but not the second.
 
       --   cspice_wnelmd returns TRUE or FALSE if a value exists in a
            window.
 
       --   cspice_wnexpd expands the size of the intervals in a window.
 
       --   cspice_wnextd extracts a window's endpoints .
 
       --   cspice_wnfild fills gaps between intervals in a window.
 
       --   cspice_wnfltd filter/removes small intervals from a window.
 
       --   cspice_wnincd determines if an interval exists within a window.
 
       --   cspice_wninsd inserts an interval into a window.
 
       --   cspice_wnreld compares two windows. Comparison operations
            available, equality '=', inequality '<>', subset '<=' and '>=',
            proper subset '<' and '>'.
 
       --   cspice_wnunid calculates the union of two windows.
 
 
Lesson 7: Utility and Constants Routines
===========================================================================
 
 
Task Statement
--------------------------------------------------------
 
   Write an interactive program to convert values between various units.
   Demonstrate the flexibility of the unit conversion routine, the string
   equality function, and show the version ID function.
 
 
Learning Goals
--------------------------------------------------------
 
   Mice provides several routines to perform commonly needed tasks. Among
   these:
 
       --   convert values between unit expressions
 
       --   identify the toolkit version
 
   Mice also includes a set of functions that return constant values often
   used in astrodynamics, time calculations, and geometry.
 
 
Code Solution
--------------------------------------------------------
 
      function units()
 
         %
         % Display the Toolkit version string with a
         % cspice_tkvrsn call.
         %
         vers = cspice_tkvrsn( 'TOOLKIT' );
         disp( ['Convert demo program compiled against CSPICE Toolkit ' ...
                                                                    vers] )
 
         %
         % The user first inputs the name of a unit of measure.
         % Send the name through TOSTAN for de-aliasing.
         %
         funits = input( 'From Units : ', 's' );
         funits = tostan( funits );
 
         %
         % Input a double precision value to express in a new
         % unit format.
         %
         fvalue = input( 'From Value : ' );
 
         %
         % Now the user inputs the name of the output units.
         % Again we send the units name through TOSTAN for
         % de-aliasing.
         %
         tunits = input( 'To Units   : ', 's' );
         tunits = tostan( tunits );
 
         tvalue = cspice_convrt( fvalue, funits, tunits );
         fprintf( '%12.6f %s\n', tvalue, tunits )
 
 
      function value = tostan( alias )
 
         value = alias;
 
         %
         % As a convenience, let's alias a few common terms
         % to their appropriate counterpart. Use strcmpi
         % to compare strings. The comparison ignores
         % letter case and trailing/leading spaces. NOTE: the SWITCH
         % statement performs the same function as the multiple
         % 'if' blocks. SWITCH was not used in order to demonstrate
         % the strcmpi call.
         %
 
         if ( strcmpi( alias, 'meter') )
 
               %
               % First, a 'meter' by any other name is a
               % 'METER' and smells as sweet ...
               %
               value = 'METERS';
 
         elseif ( strcmpi( alias, 'klicks'    ) || ...
                  strcmpi( alias, 'kilometers') || ...
                  strcmpi( alias, 'kilometer' )     )
 
               %
               % ... 'klicks' and 'KILOMETERS' and 'KILOMETER'
               % identifies 'KM'....
               %
               value = 'KM';
 
         elseif ( strcmpi( alias, 'secs') )
 
               %
               % ... 'secs' to 'SECONDS'.
               %
               value = 'SECONDS';
 
         elseif ( strcmpi( alias, 'miles') )
 
               %
               % ... and finally 'miles' to 'STATUTE_MILES'.
               % Normal people think in statute miles.
               % Only sailors think in nautical miles - one
               % minute of arc at the equator.
               %
               value = 'STATUTE_MILES';
 
         end
 
         %
         % Much better. Now return. If the input matched
         % none of the aliases, this function did nothing.
         %
 
 
Run the code example
 
   Run a few conversions through the application to ensure it works. The
   intro banner gives us the Toolkit version against which the application
   was linked:
 
      Convert demo program compiled against CSPICE Toolkit CSPICE_N0066
      From Units : klicks
      From Value : 3
      To Units   : miles
          1.864114 STATUTE_MILES
 
   Now we know. Three kilometers equals 1.864 miles.
 
   Legend states Pheidippides ran from the Marathon Plain to Athens. The
   modern marathon race (inspired by this event) spans 26.2 miles. How far
   in kilometers?
 
      Convert demo program compiled against CSPICE Toolkit CSPICE_N0066
      From Units : miles
      From Value : 26.2
      To Units   : km
         42.164813 km
 
 
Task Statement
--------------------------------------------------------
 
   Write a program to output Mice constants and use those constants to
   calculate some rudimentary values.
 
 
Code Solution
--------------------------------------------------------
 
      function xconst();
 
         %
         % All the function have the same calling sequence:
         %
         %    VALUE = function_name
         %
         %    some_procedure( function_name )
         %
         % First a simple example using the seconds per day
         % constant...
         %
         fprintf( ['Number of (S)econds (P)er (D)ay         : ', ...
                   '%19.12f\n'], cspice_spd                    )
 
         %
         % ...then show the value of degrees per radian, 180/Pi...
         %
         fprintf( ['Number of (D)egrees (P)er (R)adian      : ', ...
                   '%19.16f\n'], cspice_dpr                    )
 
         %
         % ...and the inverse, radians per degree, Pi/180.
         % It is obvious cspice_dpr() equals 1.d/cspice_rpd(), or
         % more simply cspice_dpr() * cspice_rpd() equals 1
         %
         fprintf( ['Number of (R)adians (P)er (D)egree      : ', ...
                   '%19.16f\n'], cspice_rpd                    )
 
         %
         % What's the value for the astrophysicist's favorite
         % physical constant (in a vacuum)?
         %
         fprintf( ['Speed of light in KM per second         : ', ...
                   '%19.12f\n'], cspice_clight                 )
 
         %
         % How long (in Julian days) from the J2000 epoch to the
         % J2100 epoch?
         %
         fprintf(  'Number of days between epochs J2000\n' )
         fprintf( ['  and J2100                             : ', ...
                   '%19.12f\n'], cspice_j2100 - cspice_j2000   )
 
         %
         % Redo the calculation returning seconds...
         %
         fprintf(  'Number of seconds between epochs\n' )
         fprintf( ['  J2000 and J2100                       : ', ...
                   '%19.5f\n'],                                  ...
                   cspice_spd * (cspice_j2100 - cspice_j2000)  )
 
         %
         % ...then tropical years.
         %
         fprintf(  'Number of tropical years between\n' )
         fprintf( ['  epochs J2000 and J2100                : ', ...
                   '%19.12f\n'],  (cspice_spd/cspice_tyear)      ...
                                * (cspice_j2100 - cspice_j2000))
 
         %
         % Finally, how can I convert a radian value to degrees.
         %
         fprintf( ['Number of degrees in Pi/2 radians of arc: ', ...
                   '%19.16f\n'], cspice_halfpi  * cspice_dpr   )
 
         %
         % and degrees to radians.
         %
         fprintf( ['Number of radians in 250 degrees of arc : ', ...
                   '%19.16f\n'], 250. * cspice_rpd             )
 
 
Run the code example
 
      Number of (S)econds (P)er (D)ay         :  86400.000000000000
      Number of (D)egrees (P)er (R)adian      : 57.2957795130823229
      Number of (R)adians (P)er (D)egree      :  0.0174532925199433
      Speed of light in KM per second         : 299792.457999999984
      Number of days between epochs J2000
        and J2100                             :  36525.000000000000
      Number of seconds between epochs
        J2000 and J2100                       :    3155760000.00000
      Number of tropical years between
        epochs J2000 and J2100                :    100.002135902909
      Number of degrees in Pi/2 radians of arc: 90.0000000000000000
      Number of radians in 250 degrees of arc :  4.3633231299858242
 
 
Related Routines
--------------------------------------------------------
 
       --   cspice_b1900 : Julian Date of the epoch Besselian Date 1900.0
 
       --   cspice_b1950 : Julian date of the epoch Besselian Date 1950.0
 
       --   cspice_j1900 : Julian date of 1900 JAN 0.5 this corresponds to
            calendar date 1899 DEC 31 12:00:00
 
       --   cspice_j1950 : Julian date of 1950 JAN 1.0 this corresponds to
            calendar date 1950 JAN 01 00:00:00
 
       --   cspice_twopi : double precision value of 2 * Pi
 
       --   cspice_pi : double precision value of Pi
 
       --   cspice_jyear : seconds per Julian year (365.25 Julian days)
 
